(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "RP2040 Minimal Design Example")
		(date "2020-07-13")
		(rev "REV1")
		(company "Raspberry Pi (Trading) Ltd")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0.051)
		(solder_mask_min_width 0.09)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 100 100)
		(grid_origin 121.59 74)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "VBUS")
	(net 3 "/XIN")
	(net 4 "/XOUT")
	(net 5 "+3V3")
	(net 6 "+1V1")
	(net 7 "Net-(J1-Pad4)")
	(net 8 "/~{USB_BOOT}")
	(net 9 "/GPIO15")
	(net 10 "/GPIO14")
	(net 11 "/GPIO13")
	(net 12 "/GPIO12")
	(net 13 "/GPIO11")
	(net 14 "/GPIO10")
	(net 15 "/GPIO9")
	(net 16 "/GPIO8")
	(net 17 "/GPIO7")
	(net 18 "/GPIO6")
	(net 19 "/GPIO5")
	(net 20 "/GPIO4")
	(net 21 "/GPIO3")
	(net 22 "/GPIO2")
	(net 23 "/GPIO1")
	(net 24 "/GPIO0")
	(net 25 "/GPIO29_ADC3")
	(net 26 "/GPIO28_ADC2")
	(net 27 "/GPIO27_ADC1")
	(net 28 "/GPIO26_ADC0")
	(net 29 "/GPIO25")
	(net 30 "/GPIO24")
	(net 31 "/GPIO23")
	(net 32 "/GPIO22")
	(net 33 "/GPIO21")
	(net 34 "/GPIO20")
	(net 35 "/GPIO19")
	(net 36 "/GPIO18")
	(net 37 "/GPIO17")
	(net 38 "/GPIO16")
	(net 39 "/RUN")
	(net 40 "/SWD")
	(net 41 "/SWCLK")
	(net 42 "/QSPI_SS")
	(net 43 "Net-(R3-Pad2)")
	(net 44 "Net-(R4-Pad2)")
	(net 45 "/QSPI_SD3")
	(net 46 "/QSPI_SCLK")
	(net 47 "/QSPI_SD0")
	(net 48 "/QSPI_SD2")
	(net 49 "/QSPI_SD1")
	(net 50 "/USB_D+")
	(net 51 "/USB_D-")
	(net 52 "Net-(C3-Pad1)")
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 109.025 89)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RP2040_minimal:USB_Micro-B_Amphenol_10103594-0001LF_Horizontal_modified"
		(layer "F.Cu")
		(at 100 71.7 180)
		(descr "Micro USB Type B 10103594-0001LF, http://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10103594.pdf")
		(tags "USB USB_B USB_micro USB_OTG")
		(property "Reference" "J1"
			(at -5.365 -2.58 180)
			(layer "F.SilkS")
		)
		(property "Value" "USB_B_Micro"
			(at -0.025 3.32 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "PCB edge"
			(at -0.025 1.12 180)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at -0.025 -1.13 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.3 -2.825 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "VBUS")
		)
		(pad "2" smd rect
			(at -0.65 -2.825 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "/USB_D-")
		)
		(pad "3" smd rect
			(at 0 -2.825 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/USB_D+")
		)
		(pad "4" smd rect
			(at 0.65 -2.825 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(J1-Pad4)")
		)
		(pad "5" smd rect
			(at 1.3 -2.825 270)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(pad "6" smd rect
			(at -2.9875 -1.7 180)
			(size 1.825 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(pad "6" smd rect
			(at -2.9 -3.03 180)
			(size 2 1.46)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(pad "6" smd roundrect
			(at -2.725 -0.425 180)
			(size 1.3 3.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.296)
			(net 1 "GND")
		)
		(pad "6" thru_hole oval
			(at -2.725 0 270)
			(size 1.8 1.3)
			(drill oval 1.2 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "6" thru_hole oval
			(at -2.425 -3.03 270)
			(size 1.45 1.05)
			(drill oval 1.05 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "6" smd rect
			(at -0.9625 0.25 270)
			(size 2.5 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(pad "6" smd rect
			(at 0.9625 0.25 270)
			(size 2.5 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(pad "6" thru_hole oval
			(at 2.425 -3.03 270)
			(size 1.45 1.05)
			(drill oval 1.05 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "6" smd roundrect
			(at 2.725 -0.425 180)
			(size 1.3 3.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.296)
			(net 1 "GND")
		)
		(pad "6" thru_hole oval
			(at 2.725 0 270)
			(size 1.8 1.3)
			(drill oval 1.2 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "6" smd rect
			(at 2.9 -3.03 180)
			(size 2 1.46)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(pad "6" smd rect
			(at 2.9875 -1.7 180)
			(size 1.825 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "10103594.stp"
			(offset
				(xyz 0 1.2 2.2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 180)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 91.11 76.54 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J2"
			(at -2.59 -0.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/~{USB_BOOT}")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x18_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 75.87 74)
		(descr "Through hole straight pin header, 2x18, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x18 2.54mm double row")
		(property "Reference" "J3"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x18_Odd_Even"
			(at 1.27 45.51 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 21.59 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+3V3")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/GPIO0")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/GPIO1")
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/GPIO2")
		)
		(pad "9" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/GPIO3")
		)
		(pad "11" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "12" thru_hole oval
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/GPIO4")
		)
		(pad "13" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "14" thru_hole oval
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/GPIO5")
		)
		(pad "15" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "16" thru_hole oval
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/GPIO6")
		)
		(pad "17" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "18" thru_hole oval
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GPIO7")
		)
		(pad "19" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "20" thru_hole oval
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/GPIO8")
		)
		(pad "21" thru_hole oval
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "22" thru_hole oval
			(at 2.54 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/GPIO9")
		)
		(pad "23" thru_hole oval
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "24" thru_hole oval
			(at 2.54 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/GPIO10")
		)
		(pad "25" thru_hole oval
			(at 0 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "26" thru_hole oval
			(at 2.54 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/GPIO11")
		)
		(pad "27" thru_hole oval
			(at 0 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "28" thru_hole oval
			(at 2.54 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/GPIO12")
		)
		(pad "29" thru_hole oval
			(at 0 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "30" thru_hole oval
			(at 2.54 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/GPIO13")
		)
		(pad "31" thru_hole oval
			(at 0 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "32" thru_hole oval
			(at 2.54 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/GPIO14")
		)
		(pad "33" thru_hole oval
			(at 0 40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "34" thru_hole oval
			(at 2.54 40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/GPIO15")
		)
		(pad "35" thru_hole oval
			(at 0 43.18)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "36" thru_hole oval
			(at 2.54 43.18)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x18_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 104 93.515 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 4.015 0.99 90)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 103 93.515 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 3.515 0.69 90)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+1V1")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 93.515 101.2 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 96.185 82.83 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0.185 1.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 89.5 82.315 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R2"
			(at -0.015 1.7 180)
			(layer "F.SilkS")
		)
		(property "Value" "DNF"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/QSPI_SS")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x18_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 121.59 74)
		(descr "Through hole straight pin header, 2x18, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x18 2.54mm double row")
		(property "Reference" "J4"
			(at 1.27 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x18_Odd_Even"
			(at 1.27 45.51 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 21.59 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/GPIO29_ADC3")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/GPIO28_ADC2")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/GPIO27_ADC1")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/GPIO26_ADC0")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "9" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/GPIO25")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "11" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/GPIO24")
		)
		(pad "12" thru_hole oval
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "13" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/GPIO23")
		)
		(pad "14" thru_hole oval
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "15" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/GPIO22")
		)
		(pad "16" thru_hole oval
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "17" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/GPIO21")
		)
		(pad "18" thru_hole oval
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "19" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/GPIO20")
		)
		(pad "20" thru_hole oval
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "21" thru_hole oval
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/GPIO19")
		)
		(pad "22" thru_hole oval
			(at 2.54 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "23" thru_hole oval
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/GPIO18")
		)
		(pad "24" thru_hole oval
			(at 2.54 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "25" thru_hole oval
			(at 0 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/GPIO17")
		)
		(pad "26" thru_hole oval
			(at 2.54 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "27" thru_hole oval
			(at 0 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/GPIO16")
		)
		(pad "28" thru_hole oval
			(at 2.54 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "29" thru_hole oval
			(at 0 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/RUN")
		)
		(pad "30" thru_hole oval
			(at 2.54 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "31" thru_hole oval
			(at 0 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/SWD")
		)
		(pad "32" thru_hole oval
			(at 2.54 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "33" thru_hole oval
			(at 0 40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/SWCLK")
		)
		(pad "34" thru_hole oval
			(at 2.54 40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "35" thru_hole oval
			(at 0 43.18)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "36" thru_hole oval
			(at 2.54 43.18)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x18_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 108 82.85 -90)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U1"
			(at 0 -4.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "NCP1117-3.3_SOT223"
			(at 0 4.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.15 -2.3 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(pad "2" smd rect
			(at -3.15 0 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "+3V3")
		)
		(pad "2" smd rect
			(at 3.15 0 270)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "+3V3")
		)
		(pad "3" smd rect
			(at -3.15 2.3 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "VBUS")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm"
		(layer "F.Cu")
		(at 93.05 87.275)
		(descr "SOIC, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf#page=68), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at 0 3.725 0)
			(layer "F.SilkS")
		)
		(property "Value" "W25Q128JVS"
			(at 0 3.56 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.6 -1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/QSPI_SS")
		)
		(pad "2" smd roundrect
			(at -3.6 -0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/QSPI_SD1")
		)
		(pad "3" smd roundrect
			(at -3.6 0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/QSPI_SD2")
		)
		(pad "4" smd roundrect
			(at -3.6 1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(pad "5" smd roundrect
			(at 3.6 1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/QSPI_SD0")
		)
		(pad "6" smd roundrect
			(at 3.6 0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/QSPI_SCLK")
		)
		(pad "7" smd roundrect
			(at 3.6 -0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/QSPI_SD3")
		)
		(pad "8" smd roundrect
			(at 3.6 -1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_5.23x5.23mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_5.275x5.275mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 99.485 109)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 1.785 0.814 0)
			(layer "F.SilkS")
		)
		(property "Value" "27p"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Net-(C3-Pad1)")
		)
		(pad "2" smd roundrect
			(at 0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 91 82.315 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R1"
			(at 0.015 1.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/QSPI_SS")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/~{USB_BOOT}")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 100 92.515 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 2.515 -0.2 270)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 106.485 101.2)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 100.381 106.485 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at -1.585 0.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 101 93.515 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R3"
			(at -3.515 -0.09 90)
			(layer "F.SilkS")
		)
		(property "Value" "27"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/USB_D+")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "Net-(R3-Pad2)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 101.5 106.485 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0.115 -1.4 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+1V1")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 107.9375 76.5)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VBUS")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 93.515 97 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -1.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 106.485 94.6)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 3.015 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RP2040_minimal:RP2040-QFN-56"
		(layer "F.Cu")
		(at 100 100)
		(descr "QFN, 56 Pin (http://www.cypress.com/file/416486/download#page=40), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
		(tags "QFN DFN_QFN")
		(property "Reference" "U3"
			(at -3.71 -4.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "RP2040"
			(at 0 4.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.6375 -0.6375)
			(size 1.084435 1.084435)
			(layers "F.Paste")
			(roundrect_rratio 0.230535)
		)
		(pad "" smd roundrect
			(at -0.6375 0.6375)
			(size 1.084435 1.084435)
			(layers "F.Paste")
			(roundrect_rratio 0.230535)
		)
		(pad "" smd roundrect
			(at 0.6375 -0.6375)
			(size 1.084435 1.084435)
			(layers "F.Paste")
			(roundrect_rratio 0.230535)
		)
		(pad "" smd roundrect
			(at 0.6375 0.6375)
			(size 1.084435 1.084435)
			(layers "F.Paste")
			(roundrect_rratio 0.230535)
		)
		(pad "1" smd roundrect
			(at -3.4375 -2.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at -3.4375 -2.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/GPIO0")
		)
		(pad "3" smd roundrect
			(at -3.4375 -1.8)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/GPIO1")
		)
		(pad "4" smd roundrect
			(at -3.4375 -1.4)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/GPIO2")
		)
		(pad "5" smd roundrect
			(at -3.4375 -1)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/GPIO3")
		)
		(pad "6" smd roundrect
			(at -3.4375 -0.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/GPIO4")
		)
		(pad "7" smd roundrect
			(at -3.4375 -0.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/GPIO5")
		)
		(pad "8" smd roundrect
			(at -3.4375 0.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/GPIO6")
		)
		(pad "9" smd roundrect
			(at -3.4375 0.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/GPIO7")
		)
		(pad "10" smd roundrect
			(at -3.4375 1)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "11" smd roundrect
			(at -3.4375 1.4)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/GPIO8")
		)
		(pad "12" smd roundrect
			(at -3.4375 1.8)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/GPIO9")
		)
		(pad "13" smd roundrect
			(at -3.4375 2.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/GPIO10")
		)
		(pad "14" smd roundrect
			(at -3.4375 2.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/GPIO11")
		)
		(pad "15" smd roundrect
			(at -2.6 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/GPIO12")
		)
		(pad "16" smd roundrect
			(at -2.2 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/GPIO13")
		)
		(pad "17" smd roundrect
			(at -1.8 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/GPIO14")
		)
		(pad "18" smd roundrect
			(at -1.4 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/GPIO15")
		)
		(pad "19" smd roundrect
			(at -1 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(pad "20" smd roundrect
			(at -0.6 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/XIN")
		)
		(pad "21" smd roundrect
			(at -0.2 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/XOUT")
		)
		(pad "22" smd roundrect
			(at 0.2 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "23" smd roundrect
			(at 0.6 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+1V1")
		)
		(pad "24" smd roundrect
			(at 1 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/SWCLK")
		)
		(pad "25" smd roundrect
			(at 1.4 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/SWD")
		)
		(pad "26" smd roundrect
			(at 1.8 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/RUN")
		)
		(pad "27" smd roundrect
			(at 2.2 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/GPIO16")
		)
		(pad "28" smd roundrect
			(at 2.6 3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/GPIO17")
		)
		(pad "29" smd roundrect
			(at 3.4375 2.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/GPIO18")
		)
		(pad "30" smd roundrect
			(at 3.4375 2.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/GPIO19")
		)
		(pad "31" smd roundrect
			(at 3.4375 1.8)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/GPIO20")
		)
		(pad "32" smd roundrect
			(at 3.4375 1.4)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/GPIO21")
		)
		(pad "33" smd roundrect
			(at 3.4375 1)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "34" smd roundrect
			(at 3.4375 0.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/GPIO22")
		)
		(pad "35" smd roundrect
			(at 3.4375 0.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/GPIO23")
		)
		(pad "36" smd roundrect
			(at 3.4375 -0.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/GPIO24")
		)
		(pad "37" smd roundrect
			(at 3.4375 -0.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/GPIO25")
		)
		(pad "38" smd roundrect
			(at 3.4375 -1)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/GPIO26_ADC0")
		)
		(pad "39" smd roundrect
			(at 3.4375 -1.4)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/GPIO27_ADC1")
		)
		(pad "40" smd roundrect
			(at 3.4375 -1.8)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/GPIO28_ADC2")
		)
		(pad "41" smd roundrect
			(at 3.4375 -2.2)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/GPIO29_ADC3")
		)
		(pad "42" smd roundrect
			(at 3.4375 -2.6)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "43" smd roundrect
			(at 2.6 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "44" smd roundrect
			(at 2.2 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "45" smd roundrect
			(at 1.8 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+1V1")
		)
		(pad "46" smd roundrect
			(at 1.4 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Net-(R4-Pad2)")
		)
		(pad "47" smd roundrect
			(at 1 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "Net-(R3-Pad2)")
		)
		(pad "48" smd roundrect
			(at 0.6 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "49" smd roundrect
			(at 0.2 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "50" smd roundrect
			(at -0.2 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+1V1")
		)
		(pad "51" smd roundrect
			(at -0.6 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/QSPI_SD3")
		)
		(pad "52" smd roundrect
			(at -1 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/QSPI_SCLK")
		)
		(pad "53" smd roundrect
			(at -1.4 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/QSPI_SD0")
		)
		(pad "54" smd roundrect
			(at -1.8 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/QSPI_SD2")
		)
		(pad "55" smd roundrect
			(at -2.2 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/QSPI_SD1")
		)
		(pad "56" smd roundrect
			(at -2.6 -3.4375)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/QSPI_SS")
		)
		(pad "57" thru_hole circle
			(at -1.275 -1.275)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "57" thru_hole circle
			(at -1.275 0)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "57" thru_hole circle
			(at -1.275 1.275)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "57" thru_hole circle
			(at 0 -1.275)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "57" thru_hole circle
			(at 0 0)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "57" smd roundrect
			(at 0 0)
			(size 3.2 3.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.045)
			(net 1 "GND")
		)
		(pad "57" thru_hole circle
			(at 0 1.275)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "57" thru_hole circle
			(at 1.275 -1.275)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "57" thru_hole circle
			(at 1.275 0)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "57" thru_hole circle
			(at 1.275 1.275)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 96.515 109 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 2.315 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "27p"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/XIN")
		)
		(pad "2" smd roundrect
			(at 0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5"
		(layer "F.Cu")
		(at 113.97 74)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H2"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(clearance 1)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 102 93.515 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R4"
			(at -3.515 -0.39 90)
			(layer "F.SilkS")
		)
		(property "Value" "27"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/USB_D-")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Net-(R4-Pad2)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5"
		(layer "F.Cu")
		(at 113.97 117.18)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H3"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(clearance 1)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 99 92.515 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2.515 -0.51 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.17 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+1V1")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 106.485 96)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 3.015 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 98.7 107.115 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R5"
			(at 0.085 1.4 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/XOUT")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Net-(C3-Pad1)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5"
		(layer "F.Cu")
		(at 86.03 74)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H1"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(clearance 1)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5"
		(layer "F.Cu")
		(at 86.03 117.18)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H4"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(clearance 1)
		)
		(embedded_fonts no)
	)
	(footprint "RP2040_minimal:Crystal_SMD_HC49-US"
		(layer "F.Cu")
		(at 97.841 113.116)
		(descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
		(tags "SMD SMT crystal")
		(property "Reference" "Y1"
			(at 9.349 0.084 0)
			(layer "F.SilkS")
		)
		(property "Value" "ABLS-12.000MHZ-B4-T"
			(at 0 3.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.5 0)
			(size 5.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/XIN")
		)
		(pad "2" smd rect
			(at 4.5 0)
			(size 5.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(C3-Pad1)")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_HC49-SD.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 85.115 78)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 123 121)
		(end 77 121)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126 73)
		(end 126 118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 77 70)
		(end 123 70)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 74 118)
		(end 74 73)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 77 121)
		(mid 74.87868 120.12132)
		(end 74 118)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123 70)
		(mid 125.12132 70.87868)
		(end 126 73)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 74 73)
		(mid 74.87868 70.87868)
		(end 77 70)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 126 118)
		(mid 125.12132 120.12132)
		(end 123 121)
		(layer "Edge.Cuts")
	)
	(gr_text "GP1"
		(at 81.585 79.08 0)
		(layer "F.SilkS")
	)
	(gr_text "GP2"
		(at 81.585 81.62 0)
		(layer "F.SilkS")
	)
	(gr_text "GP3"
		(at 81.585 84.16 0)
		(layer "F.SilkS")
	)
	(gr_text "GP4"
		(at 81.585 86.7 0)
		(layer "F.SilkS")
	)
	(gr_text "GP5"
		(at 81.585 89.24 0)
		(layer "F.SilkS")
	)
	(gr_text "GP6"
		(at 81.585 91.78 0)
		(layer "F.SilkS")
	)
	(gr_text "GP7"
		(at 81.585 94.32 0)
		(layer "F.SilkS")
	)
	(gr_text "GP8"
		(at 81.585 96.86 0)
		(layer "F.SilkS")
	)
	(gr_text "GP9"
		(at 81.585 99.4 0)
		(layer "F.SilkS")
	)
	(gr_text "GP11"
		(at 81.585 104.48 0)
		(layer "F.SilkS")
	)
	(gr_text "GP10"
		(at 81.585 101.94 0)
		(layer "F.SilkS")
	)
	(gr_text "GP12"
		(at 81.585 107.02 0)
		(layer "F.SilkS")
	)
	(gr_text "GP13"
		(at 81.585 109.56 0)
		(layer "F.SilkS")
	)
	(gr_text "GP15"
		(at 81.585 114.64 0)
		(layer "F.SilkS")
	)
	(gr_text "GP14"
		(at 81.585 112.1 0)
		(layer "F.SilkS")
	)
	(gr_text "GP28"
		(at 118.415 76.54 0)
		(layer "F.SilkS")
	)
	(gr_text "GP27"
		(at 118.415 79.08 0)
		(layer "F.SilkS")
	)
	(gr_text "GP26"
		(at 118.415 81.62 0)
		(layer "F.SilkS")
	)
	(gr_text "GP25"
		(at 118.415 84.16 0)
		(layer "F.SilkS")
	)
	(gr_text "GP24"
		(at 118.415 86.7 0)
		(layer "F.SilkS")
	)
	(gr_text "GP23"
		(at 118.415 89.24 0)
		(layer "F.SilkS")
	)
	(gr_text "GP21"
		(at 118.415 94.32 0)
		(layer "F.SilkS")
	)
	(gr_text "GP20"
		(at 118.415 96.86 0)
		(layer "F.SilkS")
	)
	(gr_text "GP19"
		(at 118.415 99.4 0)
		(layer "F.SilkS")
	)
	(gr_text "GP17"
		(at 118.415 104.48 0)
		(layer "F.SilkS")
	)
	(gr_text "GP22"
		(at 118.415 91.78 0)
		(layer "F.SilkS")
	)
	(gr_text "GP18"
		(at 118.415 101.94 0)
		(layer "F.SilkS")
	)
	(gr_text "SWCLK"
		(at 117.9705 114.64 0)
		(layer "F.SilkS")
	)
	(gr_text "SWD"
		(at 118.415 112.1 0)
		(layer "F.SilkS")
	)
	(gr_text "GP16"
		(at 118.415 107.02 0)
		(layer "F.SilkS")
	)
	(gr_text "RUN"
		(at 118.415 109.56 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 81.585 117.18 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 118.415 117.18 0)
		(layer "F.SilkS")
	)
	(gr_text "GP29"
		(at 118.415 74 0)
		(layer "F.SilkS")
	)
	(gr_text "Outer Row GND"
		(at 84.76 95.59 270)
		(layer "F.SilkS")
	)
	(gr_text "Outer Row GND"
		(at 115.24 95.59 90)
		(layer "F.SilkS")
	)
	(gr_text "Raspberry Pi RP2040"
		(at 100 116.9 0)
		(layer "F.SilkS")
	)
	(gr_text "\nUSB_BOOT"
		(at 92.38 78.1 0)
		(layer "F.SilkS")
	)
	(gr_text "GP0"
		(at 81.585 76.54 0)
		(layer "F.SilkS")
	)
	(gr_text "Minimal Design Example  REV1"
		(at 100 118.8 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 91.1 71.7 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 81.585 74 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "VBUS")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 2)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 108 78) (xy 106.1 78) (xy 106.1 81.6) (xy 101.7 81.6) (xy 101.7 75.8) (xy 104.3 75.8) (xy 104.3 75)
				(xy 108 75)
			)
		)
	)
	(zone
		(net 6)
		(net_name "+1V1")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads yes
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 102 98.2) (xy 98.4 98.2) (xy 98.4 101.6) (xy 101 101.6) (xy 101 102.4) (xy 100.2 102.4) (xy 100.2 102.2)
				(xy 97.8 102.2) (xy 97.8 97.8) (xy 100.6 97.8) (xy 100.6 97.6) (xy 101 97.6) (xy 101 97.2) (xy 102 97.2)
			)
		)
	)
	(zone
		(net 5)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.15)
		)
		(min_thickness 0.15)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 102.8 102.8) (xy 97.2 102.8) (xy 97.2 97.2) (xy 100 97.2) (xy 100.8 97.2) (xy 102.8 97.2)
			)
		)
	)
	(zone
		(net 5)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.3)
		)
		(polygon
			(pts
				(xy 125.5 120.5) (xy 74.5 120.5) (xy 74.5 70.5) (xy 125.5 70.5)
			)
		)
		(polygon
			(pts
				(xy 120.32 74) (xy 111.43 82.89) (xy 111.43 92.415) (xy 105.715 98.13) (xy 103.81 98.13) (xy 103.81 103.845)
				(xy 96.19 103.845) (xy 96.19 98.13) (xy 93.015 98.13) (xy 86.665 91.78) (xy 86.665 83.525) (xy 79.68 76.54)
				(xy 78.41 76.54) (xy 78.41 114.64) (xy 79.68 114.64) (xy 87.3 107.02) (xy 101.905 107.02) (xy 102.54 107.655)
				(xy 113.335 107.655) (xy 120.32 114.64) (xy 121.59 114.64) (xy 121.59 74)
			)
		)
		(polygon
			(pts
				(xy 98.8 76.2) (xy 98.8 85.2) (xy 88.4 85.2) (xy 87.1 86.4) (xy 87.1 90.4) (xy 88.6 91.8) (xy 92.1 91.8)
				(xy 97.1 96.8) (xy 101.1 96.8) (xy 101.1 92.2) (xy 102.9 92.2) (xy 102.9 83) (xy 101.7 81.8) (xy 101.7 76.2)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 105.99 108.6) (xy 105.99 116) (xy 89.59 116) (xy 89.59 106.7) (xy 96.69 106.7) (xy 98.79 104.6)
				(xy 99.99 104.6) (xy 99.99 108.6)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.3)
		)
		(polygon
			(pts
				(xy 125.5 120.5) (xy 74.5 120.5) (xy 74.5 70.5) (xy 125.5 70.5)
			)
		)
	)
	(embedded_fonts no)
)
